\doxysection{rtr\+\_\+bgpsec\+\_\+nlri Struct Reference}
\hypertarget{structrtr__bgpsec__nlri}{}\label{structrtr__bgpsec__nlri}\index{rtr\_bgpsec\_nlri@{rtr\_bgpsec\_nlri}}


This struct contains the Network Layer Reachability Information (NLRI).  




{\ttfamily \#include $<$bgpsec.\+h$>$}

\doxysubsubsection*{Data Fields}
\begin{DoxyCompactItemize}
\item 
uint16\+\_\+t \mbox{\hyperlink{group__mod__bgpsec__h_ga8fdf7a52fdd3292161b9b0a211377417}{afi}}
\item 
uint8\+\_\+t \mbox{\hyperlink{group__mod__bgpsec__h_ga814cbd22dd2c801137b9a9a7f0a70bb6}{safi}}
\item 
uint8\+\_\+t \mbox{\hyperlink{group__mod__bgpsec__h_gacb97c8e9530cb198806774905ca03e54}{nlri\+\_\+len}}
\item 
uint8\+\_\+t \texorpdfstring{$\ast$}{*} \mbox{\hyperlink{group__mod__bgpsec__h_gaeb1c62458cc35831b9ce13c00b7dd011}{nlri}}
\end{DoxyCompactItemize}


\doxysubsection{Detailed Description}
This struct contains the Network Layer Reachability Information (NLRI). 

The NLRI consists of a prefix and its length. 
\begin{DoxyParams}{Parameters}
{\em afi} & The Address Family Identifier. \\
\hline
{\em safi} & The Subsequent Address Family Identifier. \\
\hline
{\em nlri\+\_\+len} & The length of the nlri in bits. \\
\hline
{\em nlri} & The Network Layer Reachability Information. Trailing bits must be set to 0. \\
\hline
\end{DoxyParams}


The documentation for this struct was generated from the following file\+:\begin{DoxyCompactItemize}
\item 
rtrlib/bgpsec/\mbox{\hyperlink{bgpsec_8h}{bgpsec.\+h}}\end{DoxyCompactItemize}
